**Project Name:**

**Checklist No. …………**

**Make: j**

**Checklist for Equipment Inspection**

**Project Code: Date:**

**Model:**

**Hired Contractor**

****

| Equipment Name & Number: | | **7-CONCRETE PUMP** & | | | |
| --- | --- | --- | --- | --- | --- |
| **Note:** Please write Yes or No in the given box and if some comments write in remarks column. | | | | | |
| **SN.** | **Description** | |  | **Yes/No** | **Remarks** |
| 1. | Concrete pump should be physically in good condition. | | # |  |  |
| 2. | No damage in tire (Bolts, crack, cuts & air pressure, etc.). | | # |  |  |
| 3. | Outrigger should be free from damages. | | # |  |  |
| 4. | Dangerous or moving part should be covered with fix guard. | | # |  |  |
| 5. | Panel/switch board should be covered properly. | |  |  |  |
| 6. | Emergency stop button should be mushroom headed with red colour. | | # |  |  |
| 7. | Concrete hopper should be in good condition. | |  |  |  |
| 8. | Suitable mesh should be kept on hopper to avoid getting in touch with moving part. | | # |  |  |
| 9. | Clamp should be proper for tight joint of pipe. | | # |  |  |
| 10. | Hook should have sufficient strength to carry self-load during shifting. | |  |  |  |
| 11. | In case of electrically operated, electrical connection should  be taken in proper manner. | | # |  |  |
| 12. | In case of electrically operated, machine should be grounded as per IS 3043:1987. | | # |  |  |
| 13. | Concrete pump should be operated by competent person. | | # |  |  |
| 14. | Concrete pipe should be free from damages. | | # |  |  |



| FIT |  | PARTIALLY FIT UNFIT | |  |  |
| --- | --- | --- | --- | --- | --- |
| Inspected By | | | Reviewed By | | |
| Name: | | | Name: | | |
| Signature with date: | | | Signature with date: | | |