**Checklist No. …………**

**Make:**

**Checklist for Equipment Inspection**


**Project Code: Date:**

**Model:**

**Hired Contractor**

****

| Equipment Name & Number: | | **36-GANTRY CRANE** & | | | |
| --- | --- | --- | --- | --- | --- |
| **Note:** Please write Yes or No in the given box and if some comments write in remarks column. | | | | | |
| **SN.** | **Description** | |  | **Yes/No** | **Remarks** |
| 1. | Machine should be physically good & Should have valid TPI certificate. | | # |  |  |
| 2. | SWL should be visible on either side. | | # |  |  |
| 3. | Walkaway should be in good condition and free from obstruction. | |  |  |  |
| 4. | Access ladder should be provided with cage. | | # |  |  |
| 5. | Proximity sensor should be in working condition. | | # |  |  |
| 6. | Operator cabin should be in good condition and clean. | | # |  |  |
| 7. | Wire sling should be free from damage. | | # |  |  |
| 8. | Hook latch must be installed in hook. | | # |  |  |
| 9. | Guardrail system should be provided. | | # |  |  |
| 10. | Rotating part of motor should be covered. | | # |  |  |
| 11. | Wire sling drum should be under canopy. | | # |  |  |
| 12. | Audible horn should be in working condition. | | # |  |  |
| 13. | Fire extinguisher in operator cabin. | | # |  |  |
| 14. | Operator have suitable license. | | # |  |  |
| 15. | Deflection test should be carried out. | | # |  |  |



| FIT |  | PARTIALLY  UNFIT | |  |  |
| --- | --- | --- | --- | --- | --- |
| Inspected By | | | Reviewed By | | |
| Name: | | | Name: | | |
| Signature with date: | | | Signature with date: | | |