**Checklist for Equipment Inspection**

**Department:**


**Date:**

**Checklist No.**

**Opascor: Contractor**

**Model:**

| Equipment Name & Number: | |  | | | |
| --- | --- | --- | --- | --- | --- |
| **Note:** Please write Yes or No in the given box and if some comments are written in the remarks column. | | | | | |
| **SN.** | **Description** | |  | **Yes/No** | **Remarks** |
| 1. | Cylinders should be kept in trolleys. | | # |  |  |
| 2. | Always keep in an upright position. | | # |  |  |
| 3. | Properly secured. | | # |  |  |
| 4. | Valve protection cap. | | # |  |  |
| 5. | Regulator should be free from any defect. | | # |  |  |
| 6. | Pressure gauge should be in proper condition. | | # |  |  |
| 7. | Provide flash back arrestor. | | # |  |  |
| 8. | Provide industrial clips. | |  |  |  |
| 9. | House conditions should be color coded. | | # |  |  |
| 10. | Joint should be firm and free from defects, e.g., oily, rust & leakage, etc. | | # |  |  |
| 11. | Torch should be in good condition. | | # |  |  |
| 12. | Use proper PPEs for the Job, e.g., Leather hand gloves & safety goggles, etc. | | # |  |  |
| 13. | Keep a fire extinguisher at the working place. | | # |  |  |
| 14. | Provide a booth, made of fire retardant material (if reqired). | |  |  |  |
| 15. | Work carried out by a competent person. | | # |  |  |



****

| FIT |  | PARTIALLY FIT UNFIT | |  |  |
| --- | --- | --- | --- | --- | --- |
| Inspected By | | | Reviewed By | | |
| Name: | | | Name: | | |
| Signature with date: | | | Signature with date: | | |