**Project Name:**

**Checklist No. …………**

**Make:**

**Checklist for Equipment Inspection**

**Project Code: Date:**

**Model:**

**Hired Contractor**

****

| Equipment Name & Number: | | **25-LIFTING TOOLS & TACKLES** & | | | |
| --- | --- | --- | --- | --- | --- |
| **Note:** Please write Yes or No in the given box and if some comments write in remarks column. | | | | | |
| **SN.** | **Description** | |  | **Yes/No** | **Remarks** |
| 1. | Wire sling should be free from defects, e.g., corrosion, crack, cuts & oily, etc. | | # |  |  |
| 2. | Use thimble for making I-shape. | |  |  |  |
| 3. | Wire rope should be knotted with a proper clamp. | | # |  |  |
| 4. | Web sling should be free from defects, e.g., cuts, abrasion, knot, hole & oily, etc. | | # |  |  |
| 5. | I-shape should be free from damages. | | # |  |  |
| 6. | D-shackle should be in good condition and its face should not expand more than 15% of its original  shape. | | # |  |  |
| 7. | Suitable I-bolt should be used. | | # |  |  |
| 8. | Lifting tools & tackles should be used having suitable strength & capacity. | | # |  |  |
| 9. | Lifting tools & tackles should be handled and stored in a safe manner. | | # |  |  |



| FIT |  | PARTIALLY FIT UNFIT | |  |  |
| --- | --- | --- | --- | --- | --- |
| Inspected By | | | Reviewed By | | |
| Name: | | | Name: | | |
| Signature with date: | | | Signature with date: | | |