| **ACTIVITY: REDUCE THE NOISE LEVEL IN GENERATOR**  **Project : Location :**  **Sub-Contractor : Nature of work : Purpose:** To reduce the noise level in generator | | | | | |
| --- | --- | --- | --- | --- | --- |
| **Sl.**  **No** | **Procedures** | **Performed by** | | **Checked by** | |
| 1. | Silencer to be cleaned after every 10000 operational  hrs. |  |  |  |  |
| 2. | Pump / Nozzle / valve seating to be properly  maintained. |  |  |  |  |
| 3. | Monitor Noise level once in six month and perform  corrective measures, if needed. |  |  |  |  |
| **Prepared By : Approved By :**  **SE / SS : Project Manager :**  **Date : Date :** | | | | | |

