**Project Name:**

**Checklist No. …………**

**Make:**

**Checklist for Equipment Inspection**

**Project code:**


**Date:**

**Model:**

**Hired**

**Contractor**

| Equipment Name & Number: | | **14-HYDRA** & | | | |
| --- | --- | --- | --- | --- | --- |
| **Note:** Please write Yes or No in the given box and if some comments are written in the remarks column. | | | | | |
| **SN.** | **Description** | |  | **Yes/No** | **Remarks** |
| 1. | Hydra should be physically good & certified by TPI. | | # |  |  |
| 2. | No damage in tires (Bolts, crack, cuts & air pressure, etc.). | | # |  |  |
| 3. | Registration number should be written. | | # |  |  |
| 4. | Head & tail light and indicators are in working condition. | | # |  |  |
| 5. | No oil leakage in the hydraulic part. | | # |  |  |
| 6. | Safe work load (SWL) marked. | | # |  |  |
| 7. | Sling drum should be in good condition. | | # |  |  |
| 8. | Boom condition while full extension (free from damage, crack & jamming, etc.). | | # |  |  |
| 9. | Wire rope free from damage. | | # |  |  |
| 10. | Hoist limit switch. | | # |  |  |
| 11. | Safety latch in hook. | | # |  |  |
| 12. | Safe load indicator should be in working condition. | | # |  |  |
| 13. | Front & reverse horn. | | # |  |  |
| 14. | Fire extinguisher in operator cabin. | | # |  |  |
| 15. | Operators should have a valid license (heavy duty). | | # |  |  |
| 16. | Load chart available in operator cabin. | |  |  |  |



****

| FIT |  | PARTIALLY FIT UNFIT | |  |  |
| --- | --- | --- | --- | --- | --- |
| Inspected By | | | Reviewed By | | |
| Name: | | | Name: | | |
| Signature with date: | | | Signature with date: | | |